# 0Deg50Rpm

1. Description
2. General
3. Geometry
4. Particles
5. Contacts
6. Bonds
7. Selections

# Description

# General

gravity: x = 0 m/s², y = 0 m/s², z = -9.81 m/s²

## materials

Bulk Corn: poisson = 0.32, shear_mod = 2.3e+07 Pa, density = 1178 kg/m³, work function = 0 eV, material type = Bulk
Steel: poisson = 0.3, shear_mod = 7e+10 Pa, density = 7800 kg/m³, work function = 0 eV, material type = Equipment

## energy

total: -93.5197 J

## Simulation Properties

# Geometry

## domain

min: x = -1115.67 mm, y = -46.1792 mm, z = -390.927 mm
max: x = 1168.75 mm, y = 555.621 mm, z = 468.208 mm

## Houshing

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2212
nodes: 1106
type: Physical
volume: volume
bounding box:
lower: x = -942.275 mm, y = 59.7208 mm, z = -282.497 mm
upper: x = 1057.72 mm, y = 449.721 mm, z = 53.9962 mm
material: Steel
shape: cad_geometry

## End Flange2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = -942.275 mm, y = 59.7208 mm, z = -309.928 mm
upper: x = -937.275 mm, y = 449.721 mm, z = 53.9962 mm
material: Steel
shape: cad_geometry

## Flange Outlet

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 128
nodes: 64
type: Physical
volume: volume
bounding box:
lower: x = 616.725 mm, y = 63.7208 mm, z = -382.504 mm
upper: x = 998.725 mm, y = 445.721 mm, z = -378.504 mm
material: Steel
shape: cad_geometry

## End Flange1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = 1052.72 mm, y = 59.7208 mm, z = -309.928 mm
upper: x = 1057.72 mm, y = 449.721 mm, z = 53.9962 mm
material: Steel
shape: cad_geometry

## Outlet

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 216
nodes: 108
type: Physical
volume: volume
bounding box:
lower: x = 657.725 mm, y = 104.721 mm, z = -378.504 mm
upper: x = 957.725 mm, y = 404.721 mm, z = -178.504 mm
material: Steel
shape: cad_geometry

## Bearing2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3420
nodes: 1702
type: Physical
volume: surface
bounding box:
lower: x = 1063.92 mm, y = 149.721 mm, z = -221.004 mm
upper: x = 1146.36 mm, y = 359.721 mm, z = -11.0038 mm
material: Steel
shape: cad_geometry

## End Plate2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = -948.275 mm, y = 59.7208 mm, z = -309.928 mm
upper: x = -942.275 mm, y = 449.721 mm, z = 53.9962 mm
material: Steel
shape: cad_geometry

## End Plate1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = 1057.72 mm, y = 59.7208 mm, z = -309.928 mm
upper: x = 1063.72 mm, y = 449.721 mm, z = 53.9962 mm
material: Steel
shape: cad_geometry

## Cover

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 464
nodes: 232
type: Physical
volume: volume
bounding box:
lower: x = -993.275 mm, y = 59.7208 mm, z = 53.9962 mm
upper: x = 1106.72 mm, y = 449.721 mm, z = 57.9962 mm
material: Steel
shape: cad_geometry

## Hopper4

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 124
nodes: 64
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 4.72076 mm, z = 57.9962 mm
upper: x = -548.275 mm, y = 108.601 mm, z = 458.966 mm
material: Steel
shape: cad_geometry

## Hopper3

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 132
nodes: 68
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 4.72076 mm, z = 57.9962 mm
upper: x = -844.697 mm, y = 504.721 mm, z = 459.785 mm
material: Steel
shape: cad_geometry

## Hopper2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 116
nodes: 60
type: Physical
volume: volume
bounding box:
lower: x = -548.275 mm, y = 4.72076 mm, z = 57.9962 mm
upper: x = -544.275 mm, y = 504.721 mm, z = 457.996 mm
material: Steel
shape: cad_geometry

## Hopper1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 316
nodes: 159
type: Physical
volume: volume
bounding box:
lower: x = -1093.28 mm, y = -40.2792 mm, z = 57.9962 mm
upper: x = -499.275 mm, y = 549.721 mm, z = 458.966 mm
material: Steel
shape: cad_geometry

## Bearing1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3249
nodes: 1652
type: Physical
volume: surface
bounding box:
lower: x = -1030.59 mm, y = 149.721 mm, z = -221.004 mm
upper: x = -948.147 mm, y = 359.721 mm, z = -11.0038 mm
material: Steel
shape: cad_geometry

## Screw

transform: [1, -3.5578e-06, -3.47507e-06, 5.03992e-07] [1.22966e-06, -0.500169, 0.865928, 0.482786] [-4.81892e-06, -0.865928, -0.500169, 0.0468158] [0, 0, 0, 1]
translation: x = 0.000503992 mm, y = 482.786 mm, z = 46.8158 mm
euler orientation: x = -120.011 deg, y = 0.000276104 deg, z = 7.04544e-05 deg
scale: x = 1 , y = 1 , z = 1
facets: 6984
nodes: 3494
type: Physical
volume: volume
bounding box:
lower: x = -1031.15 mm, y = 105.478 mm, z = -265.191 mm
upper: x = 1118.85 mm, y = 404.382 mm, z = 33.7197 mm
material: Steel

#### Rotation (Linear Rotation)

time: start = 0 s, end = 2 s, loop = true, loop interval = 2 s, loop until = 20 s
origin: x = -972.907 mm, y = 254.905 mm, z = -115.926 mm
moves with body: true
initial angular velocity: x = 50 rpm, y = -3.87979e-05 rpm, z = -0.000138218 rpm
angular acceleration: x = 0 rad/s², y = 0 rad/s², z = 0 rad/s²
shape: cad_geometry

## Inlet

transform: [1, 0, 0, -0.796275] [0, 1, 0, 0.254721] [0, 0, 1, 0.455996] [0, 0, 0, 1]
translation: x = -796.275 mm, y = 254.721 mm, z = 455.996 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2
nodes: 4
type: Virtual
volume: surface
bounding box:
lower: x = -1021.27 mm, y = 29.7208 mm, z = 455.996 mm
upper: x = -571.275 mm, y = 479.721 mm, z = 455.996 mm
shape: polygon
edges: 4
dimensions: side 1 = 450 mm, side 2 = 450 mm

## geometry totals

total facets: 18147
total nodes: 9109

# Particles

## Corn

material: Bulk Corn
mass: 0.000365601 kg
volume: 3.10357e-07 m³
moment of inertia: x = 2.15838e-09 kgm², y = 3.09917e-09 kgm², z = 3.10219e-09 kgm²

#### Sphere 0

name: sphere 0
position: x = -0.654128 mm, y = -0.000871011 mm, z = -0.00331493 mm
contact radius: 4 mm
physical radius: 4 mm

#### Sphere 1

name: sphere 1
position: x = 3.46199 mm, y = -0.00118944 mm, z = -3.52153e-05 mm
contact radius: 2.5 mm
physical radius: 2.5 mm

## factory - Factory

type: dynamic
completed: no
particles to create: unlimited
creation rate: 6 kg/s
creation time: 0 s
rate last changed at: 0 s
mass added since rate change: 120 kg
Max attempts to place particle: 20
section: Inlet
particles created: 262479
factory_template: type = fixed, name = Corn
size: type = random, min = 0.5, max = 1.5, scaling = radius
position: type = random
velocity: type = fixed, x = 0 m/s, y = 0 m/s, z = 0 m/s
orientation: type = random
angvel: type = fixed, x = 0 rpm, y = 0 rpm, z = 0 rpm

## Particle Totals

total number: 188542
total number of type Corn: 188542

# Contacts

## interactions

interaction1: material1 = Bulk Corn, material2 = Bulk Corn, coeff_restitution = 0, coeff_static_friction = 0.12, coeff_rolling_friction = 0
interaction2: material1 = Bulk Corn, material2 = Steel, coeff_restitution = 0, coeff_static_friction = 0.3, coeff_rolling_friction = 0

## Contact Totals

Total number: 496437
Total number of Corn <> Corn: 467632
Total number of Corn <> Houshing: 14028
Total number of Corn <> End Flange2: 27
Total number of Corn <> Flange Outlet: 0
Total number of Corn <> End Flange1: 0
Total number of Corn <> Outlet: 1
Total number of Corn <> Bearing2: 0
Total number of Corn <> End Plate2: 203
Total number of Corn <> End Plate1: 0
Total number of Corn <> Cover: 0
Total number of Corn <> Hopper4: 2
Total number of Corn <> Hopper3: 3
Total number of Corn <> Hopper2: 0
Total number of Corn <> Hopper1: 0
Total number of Corn <> Bearing1: 96
Total number of Corn <> Screw: 14445

# Bonds

## bond totals

total number of bonds: 0
total number of intact bonds: 0
total number of broken bonds: 0
total intact bond number of Corn <> Corn: 0
total broken bond number of Corn <> Corn: 0

# Selections

no selection groups added to browser