# 45Deg50Rpm

1. Description
2. General
3. Geometry
4. Particles
5. Contacts
6. Bonds
7. Selections

# Description

# General

gravity: x = 0 m/s², y = 0 m/s², z = -9.81 m/s²

## materials

Bulk Corn: poisson = 0.32, shear_mod = 2.3e+07 Pa, density = 1178 kg/m³, work function = 0 eV, material type = Bulk
Steel: poisson = 0.3, shear_mod = 7e+10 Pa, density = 7800 kg/m³, work function = 0 eV, material type = Equipment

## energy

total: -22.0566 J

## Simulation Properties

# Geometry

## domain

min: x = -1115.41 mm, y = -46.1792 mm, z = -557.862 mm
max: x = 1142.2 mm, y = 555.621 mm, z = 511.697 mm

## 20 deg_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = 958.713 mm, y = 59.7208 mm, z = 137.006 mm
upper: x = 1087.88 mm, y = 449.721 mm, z = 480.693 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 128
nodes: 64
type: Physical
volume: volume
bounding box:
lower: x = 696.93 mm, y = 63.7208 mm, z = -80.3134 mm
upper: x = 1057.26 mm, y = 445.721 mm, z = 54.0971 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2212
nodes: 1106
type: Physical
volume: volume
bounding box:
lower: x = -915.974 mm, y = 59.7208 mm, z = -518.777 mm
upper: x = 1078.22 mm, y = 449.721 mm, z = 480.693 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_3

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 464
nodes: 232
type: Physical
volume: volume
bounding box:
lower: x = -965.267 mm, y = 59.7208 mm, z = -220.79 mm
upper: x = 1009.46 mm, y = 449.721 mm, z = 501.211 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_4

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 216
nodes: 108
type: Physical
volume: volume
bounding box:
lower: x = 667.054 mm, y = 104.721 mm, z = -62.5318 mm
upper: x = 1017.37 mm, y = 404.721 mm, z = 228.013 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_5

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 94
nodes: 49
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 404.721 mm, z = -168.301 mm
upper: x = -546.789 mm, y = 508.614 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_6

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 80
nodes: 42
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 404.721 mm, z = -66.2268 mm
upper: x = -544.275 mm, y = 508.47 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_7

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 132
nodes: 68
type: Physical
volume: volume
bounding box:
lower: x = -1051.72 mm, y = 4.72076 mm, z = -169.472 mm
upper: x = -829.011 mm, y = 504.721 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_8

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 96
nodes: 50
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 0.827559 mm, z = -168.301 mm
upper: x = -546.789 mm, y = 104.721 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_9

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 80
nodes: 42
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 0.971738 mm, z = -66.2268 mm
upper: x = -544.275 mm, y = 104.721 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_10

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 84
nodes: 44
type: Physical
volume: volume
bounding box:
lower: x = -547.103 mm, y = 4.72076 mm, z = -64.8743 mm
upper: x = -540.275 mm, y = 504.721 mm, z = 203.996 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_11

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = -915.974 mm, y = 59.7208 mm, z = -545.324 mm
upper: x = -786.806 mm, y = 449.721 mm, z = -201.637 mm
material: Steel
shape: cad_geometry

## 20 deg_Body_12

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 192
nodes: 96
type: Physical
volume: volume
bounding box:
lower: x = -1093.28 mm, y = -40.2792 mm, z = 203.996 mm
upper: x = -499.275 mm, y = 549.721 mm, z = 207.996 mm
material: Steel
shape: cad_geometry

## cover_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = -921.612 mm, y = 59.7208 mm, z = -547.376 mm
upper: x = -791.505 mm, y = 449.721 mm, z = -203.347 mm
material: Steel
shape: cad_geometry

## cover_Body_1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = 963.411 mm, y = 59.7208 mm, z = 138.716 mm
upper: x = 1093.52 mm, y = 449.721 mm, z = 482.745 mm
material: Steel
shape: cad_geometry

## ucf2_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3249
nodes: 1652
type: Physical
volume: surface
bounding box:
lower: x = -956.044 mm, y = 149.721 mm, z = -471.143 mm
upper: x = -827.437 mm, y = 359.721 mm, z = -266.435 mm
material: Steel
shape: cad_geometry

## Inlet

transform: [1, 0, 0, -0.796275] [0, 1, 0, 0.254721] [0, 0, 1, 0.205996] [0, 0, 0, 1]
translation: x = -796.275 mm, y = 254.721 mm, z = 205.996 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2
nodes: 4
type: Virtual
volume: surface
bounding box:
lower: x = -1021.27 mm, y = 29.7208 mm, z = 205.996 mm
upper: x = -571.275 mm, y = 479.721 mm, z = 205.996 mm
shape: polygon
edges: 4
dimensions: side 1 = 450 mm, side 2 = 450 mm

## ucf1_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3420
nodes: 1702
type: Physical
volume: surface
bounding box:
lower: x = 991.459 mm, y = 149.721 mm, z = 224.395 mm
upper: x = 1120.07 mm, y = 359.721 mm, z = 428.712 mm
material: Steel
shape: cad_geometry

## Ulir_Body_0

transform: [0.82452, 0.296167, 0.482133, -0.0510069] [-0.29617, -0.500139, 0.813723, 0.423721] [0.482131, -0.813724, -0.324658, 0.140142] [0, 0, 0, 1]
translation: x = -51.0069 mm, y = 423.721 mm, z = 140.142 mm
euler orientation: x = -121.576 deg, y = -30.3166 deg, z = -17.2277 deg
scale: x = 1 , y = 1 , z = 1
facets: 6984
nodes: 3494
type: Physical
volume: volume
bounding box:
lower: x = -952.565 mm, y = 105.478 mm, z = -472.016 mm
upper: x = 1090.04 mm, y = 404.382 mm, z = 407.848 mm
material: Steel

#### Rotation (Linear Rotation)

time: start = 0 s, end = 2 s, loop = true, loop interval = 2 s, loop until = 20 s
origin: x = -886.642 mm, y = 254.905 mm, z = -373.498 mm
moves with body: true
initial angular velocity: x = 46.9847 rpm, y = -3.8798e-05 rpm, z = 17.1009 rpm
angular acceleration: x = 0 rad/s², y = 0 rad/s², z = 0 rad/s²
shape: cad_geometry

## geometry totals

total facets: 18217
total nodes: 9149

# Particles

## Corn

material: Bulk Corn
mass: 0.000365601 kg
volume: 3.10357e-07 m³
moment of inertia: x = 2.15838e-09 kgm², y = 3.09917e-09 kgm², z = 3.10219e-09 kgm²

#### Sphere 0

name: sphere 0
position: x = -0.654128 mm, y = -0.000871011 mm, z = -0.00331493 mm
contact radius: 4 mm
physical radius: 4 mm

#### Sphere 1

name: sphere 1
position: x = 3.46199 mm, y = -0.00118944 mm, z = -3.52153e-05 mm
contact radius: 2.5 mm
physical radius: 2.5 mm

## factory - Factory

type: dynamic
completed: no
particles to create: unlimited
creation rate: 6 kg/s
creation time: 0 s
rate last changed at: 0 s
mass added since rate change: 119.999 kg
Max attempts to place particle: 20
section: Inlet
particles created: 262456
factory_template: type = fixed, name = Corn
size: type = random, min = 0.5, max = 1.5, scaling = radius
position: type = random
velocity: type = fixed, x = 0 m/s, y = 0 m/s, z = 0 m/s
orientation: type = random
angvel: type = fixed, x = 0 rpm, y = 0 rpm, z = 0 rpm

## Particle Totals

total number: 130114
total number of type Corn: 130114

# Contacts

## interactions

interaction1: material1 = Bulk Corn, material2 = Bulk Corn, coeff_restitution = 0, coeff_static_friction = 0.12, coeff_rolling_friction = 0
interaction2: material1 = Bulk Corn, material2 = Steel, coeff_restitution = 0, coeff_static_friction = 0.3, coeff_rolling_friction = 0

## Contact Totals

Total number: 288336
Total number of Corn <> Corn: 269614
Total number of Corn <> 20 deg_Body_0: 0
Total number of Corn <> 20 deg_Body_1: 0
Total number of Corn <> 20 deg_Body_2: 9543
Total number of Corn <> 20 deg_Body_3: 11
Total number of Corn <> 20 deg_Body_4: 5
Total number of Corn <> 20 deg_Body_5: 0
Total number of Corn <> 20 deg_Body_6: 8
Total number of Corn <> 20 deg_Body_7: 13
Total number of Corn <> 20 deg_Body_8: 2
Total number of Corn <> 20 deg_Body_9: 10
Total number of Corn <> 20 deg_Body_10: 18
Total number of Corn <> 20 deg_Body_11: 19
Total number of Corn <> 20 deg_Body_12: 10
Total number of Corn <> cover_Body_0: 222
Total number of Corn <> cover_Body_1: 0
Total number of Corn <> ucf2_Body_0: 243
Total number of Corn <> ucf1_Body_0: 0
Total number of Corn <> Ulir_Body_0: 8618

# Bonds

## bond totals

total number of bonds: 0
total number of intact bonds: 0
total number of broken bonds: 0
total intact bond number of Corn <> Corn: 0
total broken bond number of Corn <> Corn: 0

# Selections

no selection groups added to browser