# 45Deg50Rpm

1. Description
2. General
3. Geometry
4. Particles
5. Contacts
6. Bonds
7. Selections

# Description

# General

gravity: x = 0 m/s², y = 0 m/s², z = -9.81 m/s²

## materials

Bulk Corn: poisson = 0.32, shear_mod = 2.3e+07 Pa, density = 1178 kg/m³, work function = 0 eV, material type = Bulk
Steel: poisson = 0.3, shear_mod = 7e+10 Pa, density = 7800 kg/m³, work function = 0 eV, material type = Equipment

## energy

total: 100.09 J

## Simulation Properties

# Geometry

## domain

min: x = -1112.79 mm, y = -46.1792 mm, z = -504.969 mm
max: x = 877.787 mm, y = 555.621 mm, z = 1242.56 mm

## 45 deg_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 216
nodes: 108
type: Physical
volume: volume
bounding box:
lower: x = 472.898 mm, y = 104.721 mm, z = 599.286 mm
upper: x = 826.451 mm, y = 404.721 mm, z = 952.84 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2212
nodes: 1106
type: Physical
volume: volume
bounding box:
lower: x = -822.875 mm, y = 59.7208 mm, z = -463.618 mm
upper: x = 828.696 mm, y = 449.721 mm, z = 1187.95 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_2

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = 587.803 mm, y = 59.7208 mm, z = 927.084 mm
upper: x = 848.672 mm, y = 449.721 mm, z = 1187.95 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_3

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 128
nodes: 64
type: Physical
volume: volume
bounding box:
lower: x = 585.328 mm, y = 63.7208 mm, z = 567.467 mm
upper: x = 858.271 mm, y = 445.721 mm, z = 840.41 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_4

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 464
nodes: 232
type: Physical
volume: volume
bounding box:
lower: x = -861.766 mm, y = 59.7208 mm, z = -262.323 mm
upper: x = 625.987 mm, y = 449.721 mm, z = 1225.43 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_5

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 98
nodes: 51
type: Physical
volume: volume
bounding box:
lower: x = -1048.88 mm, y = 4.72076 mm, z = -156.964 mm
upper: x = -547.103 mm, y = 108.629 mm, z = 204.598 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_6

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 64
nodes: 34
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 4.72076 mm, z = 55.1678 mm
upper: x = -544.275 mm, y = 108.041 mm, z = 206.227 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_7

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 100
nodes: 52
type: Physical
volume: volume
bounding box:
lower: x = -1048.88 mm, y = 400.812 mm, z = -156.964 mm
upper: x = -547.103 mm, y = 504.721 mm, z = 204.598 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_8

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 64
nodes: 34
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 401.401 mm, z = 55.1678 mm
upper: x = -544.275 mm, y = 504.721 mm, z = 206.227 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_9

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 164
nodes: 84
type: Physical
volume: volume
bounding box:
lower: x = -822.875 mm, y = 59.7208 mm, z = -483.594 mm
upper: x = -562.006 mm, y = 449.721 mm, z = -222.725 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_10

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 132
nodes: 68
type: Physical
volume: volume
bounding box:
lower: x = -1048.28 mm, y = 4.72076 mm, z = -156.964 mm
upper: x = -756.113 mm, y = 504.721 mm, z = 206.496 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_11

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 60
nodes: 32
type: Physical
volume: volume
bounding box:
lower: x = -551.103 mm, y = 4.72076 mm, z = 55.1678 mm
upper: x = -544.275 mm, y = 504.721 mm, z = 204.072 mm
material: Steel
shape: cad_geometry

## 45 deg_Body_12

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 192
nodes: 96
type: Physical
volume: volume
bounding box:
lower: x = -1093.28 mm, y = -40.2792 mm, z = 203.996 mm
upper: x = -499.275 mm, y = 549.721 mm, z = 207.996 mm
material: Steel
shape: cad_geometry

## cover_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = -827.118 mm, y = 59.7208 mm, z = -487.837 mm
upper: x = -565.542 mm, y = 449.721 mm, z = -226.261 mm
material: Steel
shape: cad_geometry

## cover_Body_1

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 228
nodes: 114
type: Physical
volume: volume
bounding box:
lower: x = 591.338 mm, y = 59.7208 mm, z = 930.62 mm
upper: x = 852.914 mm, y = 449.721 mm, z = 1192.2 mm
material: Steel
shape: cad_geometry

## ucf2_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3445
nodes: 1748
type: Physical
volume: surface
bounding box:
lower: x = -802.703 mm, y = 149.721 mm, z = -446.505 mm
upper: x = -632.573 mm, y = 359.721 mm, z = -276.375 mm
material: Steel
shape: cad_geometry

## Inlet

transform: [1, 0, 0, -0.796275] [0, 1, 0, 0.254721] [0, 0, 1, 0.205996] [0, 0, 0, 1]
translation: x = -796.275 mm, y = 254.721 mm, z = 205.996 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 2
nodes: 4
type: Virtual
volume: surface
bounding box:
lower: x = -1021.27 mm, y = 29.7208 mm, z = 205.996 mm
upper: x = -571.275 mm, y = 479.721 mm, z = 205.996 mm
shape: polygon
edges: 4
dimensions: side 1 = 450 mm, side 2 = 450 mm

## ucf1_Body_0

transform: [1, 0, 0, 0] [0, 1, 0, 0] [0, 0, 1, 0] [0, 0, 0, 1]
translation: x = 0 mm, y = 0 mm, z = 0 mm
euler orientation: x = 0 deg, y = 0 deg, z = 0 deg
scale: x = 1 , y = 1 , z = 1
facets: 3418
nodes: 1701
type: Physical
volume: surface
bounding box:
lower: x = 641.678 mm, y = 149.721 mm, z = 997.876 mm
upper: x = 811.807 mm, y = 359.721 mm, z = 1168.01 mm
material: Steel
shape: cad_geometry

## Ulir_Body_0

transform: [0.249928, 0.612303, 0.75008, -0.423338] [-0.612314, -0.500152, 0.612307, 0.164235] [0.750072, -0.612317, 0.24992, 0.423341] [0, 0, 0, 1]
translation: x = -423.338 mm, y = 164.235 mm, z = 423.341 mm
euler orientation: x = -129.243 deg, y = -71.5716 deg, z = -37.757 deg
scale: x = 1 , y = 1 , z = 1
facets: 6982
nodes: 3493
type: Physical
volume: volume
bounding box:
lower: x = -788.713 mm, y = 105.489 mm, z = -432.128 mm
upper: x = 777.6 mm, y = 404.385 mm, z = 1134.17 mm
material: Steel

#### Rpm (Linear Rotation)

time: start = 0 s, end = 2 s, loop = true, loop interval = 2 s, loop until = 20 s
origin: x = -724.383 mm, y = 254.914 mm, z = -368.075 mm
moves with body: true
initial angular velocity: x = 35.3554 rpm, y = -0.000247337 rpm, z = 35.3552 rpm
angular acceleration: x = 0 rad/s², y = 0 rad/s², z = 0 rad/s²
shape: cad_geometry

## geometry totals

total facets: 18361
total nodes: 9219

# Particles

## Corn

material: Bulk Corn
mass: 0.000365601 kg
volume: 3.10357e-07 m³
moment of inertia: x = 2.15838e-09 kgm², y = 3.09917e-09 kgm², z = 3.10219e-09 kgm²

#### Sphere 0

name: sphere 0
position: x = -0.654128 mm, y = -0.000871011 mm, z = -0.00331493 mm
contact radius: 4 mm
physical radius: 4 mm

#### Sphere 1

name: sphere 1
position: x = 3.46199 mm, y = -0.00118944 mm, z = -3.52153e-05 mm
contact radius: 2.5 mm
physical radius: 2.5 mm

## factory - Factory

type: dynamic
completed: no
particles to create: unlimited
creation rate: 6 kg/s
creation time: 0 s
rate last changed at: 0 s
mass added since rate change: 120 kg
Max attempts to place particle: 20
section: Inlet
particles created: 262727
factory_template: type = fixed, name = Corn
size: type = random, min = 0.5, max = 1.5, scaling = radius
position: type = random
velocity: type = fixed, x = 0 m/s, y = 0 m/s, z = 0 m/s
orientation: type = random
angvel: type = fixed, x = 0 rpm, y = 0 rpm, z = 0 rpm

## Particle Totals

total number: 104521
total number of type Corn: 104521

# Contacts

## interactions

interaction1: material1 = Bulk Corn, material2 = Bulk Corn, coeff_restitution = 0, coeff_static_friction = 0.12, coeff_rolling_friction = 0
interaction2: material1 = Bulk Corn, material2 = Steel, coeff_restitution = 0, coeff_static_friction = 0.3, coeff_rolling_friction = 0

## Contact Totals

Total number: 180542
Total number of Corn <> Corn: 166840
Total number of Corn <> 45 deg_Body_0: 5
Total number of Corn <> 45 deg_Body_1: 7042
Total number of Corn <> 45 deg_Body_2: 0
Total number of Corn <> 45 deg_Body_3: 0
Total number of Corn <> 45 deg_Body_4: 53
Total number of Corn <> 45 deg_Body_5: 10
Total number of Corn <> 45 deg_Body_6: 1
Total number of Corn <> 45 deg_Body_7: 2
Total number of Corn <> 45 deg_Body_8: 4
Total number of Corn <> 45 deg_Body_9: 46
Total number of Corn <> 45 deg_Body_10: 16
Total number of Corn <> 45 deg_Body_11: 36
Total number of Corn <> 45 deg_Body_12: 5
Total number of Corn <> cover_Body_0: 656
Total number of Corn <> cover_Body_1: 0
Total number of Corn <> ucf2_Body_0: 279
Total number of Corn <> ucf1_Body_0: 0
Total number of Corn <> Ulir_Body_0: 5547

# Bonds

## bond totals

total number of bonds: 0
total number of intact bonds: 0
total number of broken bonds: 0
total intact bond number of Corn <> Corn: 0
total broken bond number of Corn <> Corn: 0

# Selections

no selection groups added to browser